Esc | Stop Tx, abort QSO, clear next-call queue
F1 | Online User's Guide (Alt: transmit Tx6)
Shift+F1 | Copyright Notice
Ctrl+F1 | About WSJT-X
F2 | Open settings window (Alt: transmit Tx2)
F3 | Display keyboard shortcuts (Alt: transmit Tx3)
F4 | Clear DX Call, DX Grid, Tx messages 1-4 (Alt: transmit Tx4)
Alt+F4 | Exit program
F5 | Display special mouse commands (Alt: transmit Tx5)
F6 | Open next file in directory (Alt: toggle "Call 1st")
Shift+F6 | Decode all remaining files in directrory
F7 | Display Message Averaging window
F11 | Move Rx frequency down 1 Hz
Ctrl+F11 | Move identical Rx and Tx frequencies down 1 Hz
Shift+F11 | Move Tx frequency down 60 Hz (FT8) or 90 Hz (FT4)
Ctrl+Shift+F11 | Move dial frequency down 2000 Hz
F12 | Move Rx frequency up 1 Hz
Ctrl+F12 | Move identical Rx and Tx frequencies up 1 Hz
Shift+F12 | Move Tx frequency up 60 Hz (FT8) or 90 Hz (FT4)
Ctrl+Shift+F12 | Move dial frequency up 2000 Hz
Alt+1-6 | Set now transmission to this number on Tab 1
Ctl+1-6 | Set next transmission to this number on Tab 1
Alt+B | Toggle "Best S+P" status
Alt+C | Toggle "Call 1st" checkbox
Alt+D | Decode again at QSO frequency
Shift+D | Full decode (both windows)
Ctrl+E | Turn on TX even/1st
Shift+E | Turn off TX even/1st
Alt+E | Erase
Ctrl+F | Edit the free text message box
Alt+G | Generate standard messages
Alt+H | Halt Tx
Ctrl+L | Lookup callsign in database, generate standard messages
Alt+M | Monitor
Alt+N | Enable Tx
Ctrl+O | Open a .wav file
Alt+O | Change operator
Alt+Q | Log QSO
Ctrl+R | Set Tx4 message to RRR (not in FT4)
Alt+R | Set Tx4 message to RR73
Alt+S | Stop monitoring
Alt+T | Toggle Tune status
Alt+Z | Clear hung decoder status