Click on | Action
--- | ---
Waterfall: | Click to set Rx frequency. Shift-click to set Tx frequency. Ctrl-click or Right-click to set Rx and Tx frequencies. Double-click to also decode at Rx frequency.
Decoded text: | Double-click to copy second callsign to Dx Call, locator to Dx Grid, change Rx and Tx frequency to decoded signal's frequency, and generate standard messages. If Hold Tx Freq is checked or first callsign in message is your own call, Tx frequency is not changed unless Ctrl is held down.
Erase button: | Click to erase QSO window. Double-click to erase QSO and Band Activity windows.